|  |  |  |
| --- | --- | --- |
|  | TTI | Year |
| Weighted Average (Peak) By Volume | 1.200698592 | 2023 |
| Weighted Average (Peak) By Volume | 1.321039409 | 2030 |

US288 between 610 and BW8 – 2024 TDM Model Run with Kirby Ext.

The Travel Time Index is calculated from 2023 H-GAC Travel Demand Model project level links. It is the ratio of the travel time during the peak period over the time required to make the same trip at free-flow speeds. The methodology used is derived from the Highway Capacity Manual, 7th Edition.  Citation: National Academies of Sciences, Engineering, and Medicine. 2022. Highway Capacity Manual 7th Edition: A Guide for Multimodal Mobility Analysis. Washington, DC: The National Academies Press.